### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.
To see the actual file transmitted to Xilinx, please click here.

software_version_and_target_device
beta | FALSE | build_version | 2708876
date_generated | Wed Jul 23 13:06:50 2025 | os_platform | WIN64
product_version | Vivado v2019.2 (64-bit) | project_id | ed98e4aae70f4d2bac1fbc34622afe46
project_iteration | 1 | random_id | 1f1b497c70e95691a8a301c69c46f316
registration_id | 1f1b497c70e95691a8a301c69c46f316 | route_design | TRUE
target_device | xc7z020 | target_family | zynq
target_package | clg400 | target_speed | -1
tool_flow | Vivado

user_environment
cpu_name | 12th Gen Intel(R) Core(TM) i5-12400F | cpu_speed | 2496 MHz
os_name | Windows Server 2016 or Windows 10 | os_release | major release (build 9200)
system_ram | 16.000 GB | total_processors | 1

vivado_usage

gui_handlers
basedialog_cancel=1 | basedialog_ok=5 | basedialog_yes=1 | cmdmsgdialog_ok=1
coretreetablepanel_core_tree_table=14 | createnewdiagramdialog_design_name=1 | filesetpanel_file_set_panel_tree=1 | flownavigatortreepanel_flow_navigator_tree=2
pacommandnames_create_top_hdl=1 | paviews_project_summary=1 | rsbapplyautomationbar_run_block_automation=2 | rsbapplyautomationbar_run_connection_automation=1
systembuilderview_add_ip=2 | systemtreeview_system_tree=1

java_command_handlers
createblockdesign=1 | createtophdl=1 | runbitgen=1

other_data
guimode=1

project_data
constraintsetcount=0 | core_container=false | currentimplrun=impl_1 | currentsynthesisrun=synth_1
default_library=xil_defaultlib | designmode=RTL | export_simulation_activehdl=0 | export_simulation_ies=0
export_simulation_modelsim=0 | export_simulation_questa=0 | export_simulation_riviera=0 | export_simulation_vcs=0
export_simulation_xsim=0 | implstrategy=Vivado Implementation Defaults | launch_simulation_activehdl=0 | launch_simulation_ies=0
launch_simulation_modelsim=0 | launch_simulation_questa=0 | launch_simulation_riviera=0 | launch_simulation_vcs=0
launch_simulation_xsim=0 | simulator_language=Mixed | srcsetcount=2 | synthesisstrategy=Vivado Synthesis Defaults
target_language=Verilog | target_simulator=XSim | totalimplruns=5 | totalsynthesisruns=5

unisim_transformation
post_unisim_transformation
bibuf=130 | bufg=1 | carry4=66 | fdre=828
fdse=20 | gnd=68 | lut1=146 | lut2=120
lut3=345 | lut4=130 | lut5=72 | lut6=183
ps7=1 | srl16e=19 | srlc32e=47 | vcc=40
pre_unisim_transformation
bibuf=130 | bufg=1 | carry4=66 | fdre=828
fdse=20 | gnd=68 | lut1=146 | lut2=120
lut3=345 | lut4=130 | lut5=72 | lut6=183
ps7=1 | srl16e=19 | srlc32e=47 | vcc=40

phys_opt_design_post_place
command_line_options
-aggressive_hold_fix=default::[not_specified] | -bram_register_opt=default::[not_specified] | -clock_opt=default::[not_specified] | -critical_cell_opt=default::[not_specified]
-critical_pin_opt=default::[not_specified] | -directive=default::[not_specified] | -dsp_register_opt=default::[not_specified] | -effort_level=default::[not_specified]
-fanout_opt=default::[not_specified] | -hold_fix=default::[not_specified] | -insert_negative_edge_ffs=default::[not_specified] | -multi_clock_opt=default::[not_specified]
-placement_opt=default::[not_specified] | -restruct_opt=default::[not_specified] | -retime=default::[not_specified] | -rewire=default::[not_specified]
-shift_register_opt=default::[not_specified] | -uram_register_opt=default::[not_specified] | -verbose=default::[not_specified] | -vhfn=default::[not_specified]

ip_statistics
IP_Integrator/1
bdsource=USER | core_container=NA | da_axi4_cnt=1 | da_ps7_cnt=1
iptotal=1 | maxhierdepth=0 | numblks=6 | numhdlrefblks=0
numhierblks=2 | numhlsblks=0 | numnonxlnxblks=0 | numpkgbdblks=0
numreposblks=4 | numsysgenblks=0 | synth_mode=OOC_per_IP | x_iplanguage=VERILOG
x_iplibrary=BlockDiagram | x_ipname=Assignment_7_BD | x_ipvendor=xilinx.com | x_ipversion=1.00.a
axi_protocol_converter_v2_1_20_axi_protocol_converter/1
c_axi_addr_width=32 | c_axi_aruser_width=1 | c_axi_awuser_width=1 | c_axi_buser_width=1
c_axi_data_width=32 | c_axi_id_width=12 | c_axi_ruser_width=1 | c_axi_supports_read=1
c_axi_supports_user_signals=0 | c_axi_supports_write=1 | c_axi_wuser_width=1 | c_family=zynq
c_ignore_id=0 | c_m_axi_protocol=2 | c_s_axi_protocol=1 | c_translation_mode=2
core_container=NA | iptotal=1 | x_ipcorerevision=20 | x_iplanguage=VERILOG
x_iplibrary=ip | x_ipname=axi_protocol_converter | x_ipproduct=Vivado 2019.2 | x_ipsimlanguage=MIXED
x_ipvendor=xilinx.com | x_ipversion=2.1
axi_timer/1
c_count_width=32 | c_family=zynq | c_gen0_assert=1 | c_gen1_assert=1
c_one_timer_only=0 | c_s_axi_addr_width=5 | c_s_axi_data_width=32 | c_trig0_assert=1
c_trig1_assert=1 | core_container=NA | iptotal=1 | x_ipcorerevision=22
x_iplanguage=VERILOG | x_iplibrary=ip | x_ipname=axi_timer | x_ipproduct=Vivado 2019.2
x_ipsimlanguage=MIXED | x_ipvendor=xilinx.com | x_ipversion=2.0
proc_sys_reset/1
c_aux_reset_high=0 | c_aux_rst_width=4 | c_ext_reset_high=0 | c_ext_rst_width=4
c_family=zynq | c_num_bus_rst=1 | c_num_interconnect_aresetn=1 | c_num_perp_aresetn=1
c_num_perp_rst=1 | core_container=NA | iptotal=1 | x_ipcorerevision=13
x_iplanguage=VERILOG | x_iplibrary=ip | x_ipname=proc_sys_reset | x_ipproduct=Vivado 2019.2
x_ipsimlanguage=MIXED | x_ipvendor=xilinx.com | x_ipversion=5.0
processing_system7_v5.5_user_configuration/1
core_container=NA | iptotal=1 | pcw_apu_clk_ratio_enable=6:2:1 | pcw_apu_peripheral_freqmhz=666.666666
pcw_armpll_ctrl_fbdiv=40 | pcw_can0_grp_clk_enable=0 | pcw_can0_peripheral_clksrc=External | pcw_can0_peripheral_enable=0
pcw_can0_peripheral_freqmhz=-1 | pcw_can1_grp_clk_enable=0 | pcw_can1_peripheral_clksrc=External | pcw_can1_peripheral_enable=0
pcw_can1_peripheral_freqmhz=-1 | pcw_can_peripheral_clksrc=IO PLL | pcw_can_peripheral_freqmhz=100 | pcw_cpu_cpu_pll_freqmhz=1333.333
pcw_cpu_peripheral_clksrc=ARM PLL | pcw_crystal_peripheral_freqmhz=33.333333 | pcw_dci_peripheral_clksrc=DDR PLL | pcw_dci_peripheral_freqmhz=10.159
pcw_ddr_ddr_pll_freqmhz=1066.667 | pcw_ddr_hpr_to_critical_priority_level=15 | pcw_ddr_hprlpr_queue_partition=HPR(0)/LPR(32) | pcw_ddr_lpr_to_critical_priority_level=2
pcw_ddr_peripheral_clksrc=DDR PLL | pcw_ddr_port0_hpr_enable=0 | pcw_ddr_port1_hpr_enable=0 | pcw_ddr_port2_hpr_enable=0
pcw_ddr_port3_hpr_enable=0 | pcw_ddr_write_to_critical_priority_level=2 | pcw_ddrpll_ctrl_fbdiv=32 | pcw_enet0_enet0_io=MIO 16 .. 27
pcw_enet0_grp_mdio_enable=1 | pcw_enet0_peripheral_clksrc=IO PLL | pcw_enet0_peripheral_enable=1 | pcw_enet0_peripheral_freqmhz=1000 Mbps
pcw_enet0_reset_enable=0 | pcw_enet1_grp_mdio_enable=0 | pcw_enet1_peripheral_clksrc=IO PLL | pcw_enet1_peripheral_enable=0
pcw_enet1_peripheral_freqmhz=1000 Mbps | pcw_enet1_reset_enable=0 | pcw_enet_reset_polarity=Active Low | pcw_fclk0_peripheral_clksrc=IO PLL
pcw_fclk1_peripheral_clksrc=IO PLL | pcw_fclk2_peripheral_clksrc=IO PLL | pcw_fclk3_peripheral_clksrc=IO PLL | pcw_fpga0_peripheral_freqmhz=50
pcw_fpga1_peripheral_freqmhz=50 | pcw_fpga2_peripheral_freqmhz=50 | pcw_fpga3_peripheral_freqmhz=50 | pcw_fpga_fclk0_enable=1
pcw_fpga_fclk1_enable=0 | pcw_fpga_fclk2_enable=0 | pcw_fpga_fclk3_enable=0 | pcw_gpio_emio_gpio_enable=0
pcw_gpio_mio_gpio_enable=1 | pcw_gpio_mio_gpio_io=MIO | pcw_gpio_peripheral_enable=0 | pcw_i2c0_grp_int_enable=0
pcw_i2c0_peripheral_enable=0 | pcw_i2c0_reset_enable=0 | pcw_i2c1_grp_int_enable=0 | pcw_i2c1_peripheral_enable=0
pcw_i2c1_reset_enable=0 | pcw_i2c_reset_polarity=Active Low | pcw_io_io_pll_freqmhz=1000.000 | pcw_iopll_ctrl_fbdiv=30
pcw_irq_f2p_mode=DIRECT | pcw_m_axi_gp0_freqmhz=50 | pcw_m_axi_gp1_freqmhz=10 | pcw_nand_cycles_t_ar=1
pcw_nand_cycles_t_clr=1 | pcw_nand_cycles_t_rc=11 | pcw_nand_cycles_t_rea=1 | pcw_nand_cycles_t_rr=1
pcw_nand_cycles_t_wc=11 | pcw_nand_cycles_t_wp=1 | pcw_nand_grp_d8_enable=0 | pcw_nand_peripheral_enable=0
pcw_nor_cs0_t_ceoe=1 | pcw_nor_cs0_t_pc=1 | pcw_nor_cs0_t_rc=11 | pcw_nor_cs0_t_tr=1
pcw_nor_cs0_t_wc=11 | pcw_nor_cs0_t_wp=1 | pcw_nor_cs0_we_time=0 | pcw_nor_cs1_t_ceoe=1
pcw_nor_cs1_t_pc=1 | pcw_nor_cs1_t_rc=11 | pcw_nor_cs1_t_tr=1 | pcw_nor_cs1_t_wc=11
pcw_nor_cs1_t_wp=1 | pcw_nor_cs1_we_time=0 | pcw_nor_grp_a25_enable=0 | pcw_nor_grp_cs0_enable=0
pcw_nor_grp_cs1_enable=0 | pcw_nor_grp_sram_cs0_enable=0 | pcw_nor_grp_sram_cs1_enable=0 | pcw_nor_grp_sram_int_enable=0
pcw_nor_peripheral_enable=0 | pcw_nor_sram_cs0_t_ceoe=1 | pcw_nor_sram_cs0_t_pc=1 | pcw_nor_sram_cs0_t_rc=11
pcw_nor_sram_cs0_t_tr=1 | pcw_nor_sram_cs0_t_wc=11 | pcw_nor_sram_cs0_t_wp=1 | pcw_nor_sram_cs0_we_time=0
pcw_nor_sram_cs1_t_ceoe=1 | pcw_nor_sram_cs1_t_pc=1 | pcw_nor_sram_cs1_t_rc=11 | pcw_nor_sram_cs1_t_tr=1
pcw_nor_sram_cs1_t_wc=11 | pcw_nor_sram_cs1_t_wp=1 | pcw_nor_sram_cs1_we_time=0 | pcw_override_basic_clock=0
pcw_pcap_peripheral_clksrc=IO PLL | pcw_pcap_peripheral_freqmhz=200 | pcw_pjtag_peripheral_enable=0 | pcw_preset_bank0_voltage=LVCMOS 3.3V
pcw_preset_bank1_voltage=LVCMOS 1.8V | pcw_qspi_grp_fbclk_enable=1 | pcw_qspi_grp_fbclk_io=MIO 8 | pcw_qspi_grp_io1_enable=0
pcw_qspi_grp_single_ss_enable=1 | pcw_qspi_grp_single_ss_io=MIO 1 .. 6 | pcw_qspi_grp_ss1_enable=0 | pcw_qspi_internal_highaddress=0xFCFFFFFF
pcw_qspi_peripheral_clksrc=IO PLL | pcw_qspi_peripheral_enable=1 | pcw_qspi_peripheral_freqmhz=200 | pcw_qspi_qspi_io=MIO 1 .. 6
pcw_s_axi_acp_freqmhz=10 | pcw_s_axi_gp0_freqmhz=10 | pcw_s_axi_gp1_freqmhz=10 | pcw_s_axi_hp0_data_width=64
pcw_s_axi_hp0_freqmhz=10 | pcw_s_axi_hp1_data_width=64 | pcw_s_axi_hp1_freqmhz=10 | pcw_s_axi_hp2_data_width=64
pcw_s_axi_hp2_freqmhz=10 | pcw_s_axi_hp3_data_width=64 | pcw_s_axi_hp3_freqmhz=10 | pcw_sd0_grp_cd_enable=1
pcw_sd0_grp_cd_io=MIO 47 | pcw_sd0_grp_pow_enable=0 | pcw_sd0_grp_wp_enable=0 | pcw_sd0_peripheral_enable=1
pcw_sd0_sd0_io=MIO 40 .. 45 | pcw_sd1_grp_cd_enable=0 | pcw_sd1_grp_pow_enable=0 | pcw_sd1_grp_wp_enable=0
pcw_sd1_peripheral_enable=0 | pcw_sdio_peripheral_clksrc=IO PLL | pcw_sdio_peripheral_freqmhz=50 | pcw_single_qspi_data_mode=x4
pcw_smc_peripheral_clksrc=IO PLL | pcw_smc_peripheral_freqmhz=100 | pcw_spi0_grp_ss0_enable=0 | pcw_spi0_grp_ss1_enable=0
pcw_spi0_grp_ss2_enable=0 | pcw_spi0_peripheral_enable=0 | pcw_spi1_grp_ss0_enable=0 | pcw_spi1_grp_ss1_enable=0
pcw_spi1_grp_ss2_enable=0 | pcw_spi1_peripheral_enable=0 | pcw_spi_peripheral_clksrc=IO PLL | pcw_spi_peripheral_freqmhz=166.666666
pcw_tpiu_peripheral_clksrc=External | pcw_tpiu_peripheral_freqmhz=200 | pcw_trace_grp_16bit_enable=0 | pcw_trace_grp_2bit_enable=0
pcw_trace_grp_32bit_enable=0 | pcw_trace_grp_4bit_enable=0 | pcw_trace_grp_8bit_enable=0 | pcw_trace_peripheral_enable=0
pcw_ttc0_clk0_peripheral_clksrc=CPU_1X | pcw_ttc0_clk0_peripheral_freqmhz=133.333333 | pcw_ttc0_clk1_peripheral_clksrc=CPU_1X | pcw_ttc0_clk1_peripheral_freqmhz=133.333333
pcw_ttc0_clk2_peripheral_clksrc=CPU_1X | pcw_ttc0_clk2_peripheral_freqmhz=133.333333 | pcw_ttc0_peripheral_enable=0 | pcw_ttc1_clk0_peripheral_clksrc=CPU_1X
pcw_ttc1_clk0_peripheral_freqmhz=133.333333 | pcw_ttc1_clk1_peripheral_clksrc=CPU_1X | pcw_ttc1_clk1_peripheral_freqmhz=133.333333 | pcw_ttc1_clk2_peripheral_clksrc=CPU_1X
pcw_ttc1_clk2_peripheral_freqmhz=133.333333 | pcw_ttc1_peripheral_enable=0 | pcw_ttc_peripheral_freqmhz=50 | pcw_uart0_baud_rate=115200
pcw_uart0_grp_full_enable=0 | pcw_uart0_peripheral_enable=0 | pcw_uart1_baud_rate=115200 | pcw_uart1_grp_full_enable=0
pcw_uart1_peripheral_enable=1 | pcw_uart1_uart1_io=MIO 48 .. 49 | pcw_uart_peripheral_clksrc=IO PLL | pcw_uart_peripheral_freqmhz=100
pcw_uiparam_ddr_adv_enable=0 | pcw_uiparam_ddr_al=0 | pcw_uiparam_ddr_bank_addr_count=3 | pcw_uiparam_ddr_bl=8
pcw_uiparam_ddr_board_delay0=0.221 | pcw_uiparam_ddr_board_delay1=0.222 | pcw_uiparam_ddr_board_delay2=0.217 | pcw_uiparam_ddr_board_delay3=0.244
pcw_uiparam_ddr_bus_width=32 Bit | pcw_uiparam_ddr_cl=7 | pcw_uiparam_ddr_clock_0_length_mm=18.8 | pcw_uiparam_ddr_clock_0_package_length=80.4535
pcw_uiparam_ddr_clock_0_propogation_delay=160 | pcw_uiparam_ddr_clock_1_length_mm=18.8 | pcw_uiparam_ddr_clock_1_package_length=80.4535 | pcw_uiparam_ddr_clock_1_propogation_delay=160
pcw_uiparam_ddr_clock_2_length_mm=18.8 | pcw_uiparam_ddr_clock_2_package_length=80.4535 | pcw_uiparam_ddr_clock_2_propogation_delay=160 | pcw_uiparam_ddr_clock_3_length_mm=18.8
pcw_uiparam_ddr_clock_3_package_length=80.4535 | pcw_uiparam_ddr_clock_3_propogation_delay=160 | pcw_uiparam_ddr_clock_stop_en=0 | pcw_uiparam_ddr_col_addr_count=10
pcw_uiparam_ddr_cwl=6 | pcw_uiparam_ddr_device_capacity=4096 MBits | pcw_uiparam_ddr_dq_0_length_mm=22.8 | pcw_uiparam_ddr_dq_0_package_length=98.503
pcw_uiparam_ddr_dq_0_propogation_delay=160 | pcw_uiparam_ddr_dq_1_length_mm=27.9 | pcw_uiparam_ddr_dq_1_package_length=68.5855 | pcw_uiparam_ddr_dq_1_propogation_delay=160
pcw_uiparam_ddr_dq_2_length_mm=22.9 | pcw_uiparam_ddr_dq_2_package_length=90.295 | pcw_uiparam_ddr_dq_2_propogation_delay=160 | pcw_uiparam_ddr_dq_3_length_mm=29.4
pcw_uiparam_ddr_dq_3_package_length=103.977 | pcw_uiparam_ddr_dq_3_propogation_delay=160 | pcw_uiparam_ddr_dqs_0_length_mm=22.8 | pcw_uiparam_ddr_dqs_0_package_length=105.056
pcw_uiparam_ddr_dqs_0_propogation_delay=160 | pcw_uiparam_ddr_dqs_1_length_mm=27.9 | pcw_uiparam_ddr_dqs_1_package_length=66.904 | pcw_uiparam_ddr_dqs_1_propogation_delay=160
pcw_uiparam_ddr_dqs_2_length_mm=22.9 | pcw_uiparam_ddr_dqs_2_package_length=89.1715 | pcw_uiparam_ddr_dqs_2_propogation_delay=160 | pcw_uiparam_ddr_dqs_3_length_mm=29.4
pcw_uiparam_ddr_dqs_3_package_length=113.63 | pcw_uiparam_ddr_dqs_3_propogation_delay=160 | pcw_uiparam_ddr_dqs_to_clk_delay_0=-0.050 | pcw_uiparam_ddr_dqs_to_clk_delay_1=-0.044
pcw_uiparam_ddr_dqs_to_clk_delay_2=-0.035 | pcw_uiparam_ddr_dqs_to_clk_delay_3=-0.100 | pcw_uiparam_ddr_dram_width=16 Bits | pcw_uiparam_ddr_ecc=Disabled
pcw_uiparam_ddr_enable=1 | pcw_uiparam_ddr_freq_mhz=533.333333 | pcw_uiparam_ddr_high_temp=Normal (0-85) | pcw_uiparam_ddr_memory_type=DDR 3 (Low Voltage)
pcw_uiparam_ddr_partno=MT41K256M16 RE-125 | pcw_uiparam_ddr_row_addr_count=15 | pcw_uiparam_ddr_speed_bin=DDR3_1066F | pcw_uiparam_ddr_t_faw=40.0
pcw_uiparam_ddr_t_ras_min=35.0 | pcw_uiparam_ddr_t_rc=48.75 | pcw_uiparam_ddr_t_rcd=7 | pcw_uiparam_ddr_t_rp=7
pcw_uiparam_ddr_train_data_eye=1 | pcw_uiparam_ddr_train_read_gate=1 | pcw_uiparam_ddr_train_write_level=1 | pcw_uiparam_ddr_use_internal_vref=0
pcw_usb0_peripheral_enable=1 | pcw_usb0_peripheral_freqmhz=60 | pcw_usb0_reset_enable=1 | pcw_usb0_reset_io=MIO 46
pcw_usb0_usb0_io=MIO 28 .. 39 | pcw_usb1_peripheral_enable=0 | pcw_usb1_peripheral_freqmhz=60 | pcw_usb1_reset_enable=0
pcw_usb_reset_polarity=Active Low | pcw_use_cross_trigger=0 | pcw_use_m_axi_gp0=1 | pcw_use_m_axi_gp1=0
pcw_use_s_axi_acp=0 | pcw_use_s_axi_gp0=0 | pcw_use_s_axi_gp1=0 | pcw_use_s_axi_hp0=0
pcw_use_s_axi_hp1=0 | pcw_use_s_axi_hp2=0 | pcw_use_s_axi_hp3=0 | pcw_wdt_peripheral_clksrc=CPU_1X
pcw_wdt_peripheral_enable=0 | pcw_wdt_peripheral_freqmhz=133.333333
processing_system7_v5_5_processing_system7/1
c_dm_width=4 | c_dq_width=32 | c_dqs_width=4 | c_emio_gpio_width=64
c_en_emio_enet0=0 | c_en_emio_enet1=0 | c_en_emio_pjtag=0 | c_en_emio_trace=0
c_fclk_clk0_buf=TRUE | c_fclk_clk1_buf=FALSE | c_fclk_clk2_buf=FALSE | c_fclk_clk3_buf=FALSE
c_gp0_en_modifiable_txn=1 | c_gp1_en_modifiable_txn=1 | c_include_acp_trans_check=0 | c_include_trace_buffer=0
c_irq_f2p_mode=DIRECT | c_m_axi_gp0_enable_static_remap=0 | c_m_axi_gp0_id_width=12 | c_m_axi_gp0_thread_id_width=12
c_m_axi_gp1_enable_static_remap=0 | c_m_axi_gp1_id_width=12 | c_m_axi_gp1_thread_id_width=12 | c_mio_primitive=54
c_num_f2p_intr_inputs=1 | c_package_name=clg400 | c_ps7_si_rev=PRODUCTION | c_s_axi_acp_aruser_val=31
c_s_axi_acp_awuser_val=31 | c_s_axi_acp_id_width=3 | c_s_axi_gp0_id_width=6 | c_s_axi_gp1_id_width=6
c_s_axi_hp0_data_width=64 | c_s_axi_hp0_id_width=6 | c_s_axi_hp1_data_width=64 | c_s_axi_hp1_id_width=6
c_s_axi_hp2_data_width=64 | c_s_axi_hp2_id_width=6 | c_s_axi_hp3_data_width=64 | c_s_axi_hp3_id_width=6
c_trace_buffer_clock_delay=12 | c_trace_buffer_fifo_size=128 | c_trace_internal_width=2 | c_trace_pipeline_width=8
c_use_axi_nonsecure=0 | c_use_default_acp_user_val=0 | c_use_m_axi_gp0=1 | c_use_m_axi_gp1=0
c_use_s_axi_acp=0 | c_use_s_axi_gp0=0 | c_use_s_axi_gp1=0 | c_use_s_axi_hp0=0
c_use_s_axi_hp1=0 | c_use_s_axi_hp2=0 | c_use_s_axi_hp3=0 | core_container=NA
iptotal=1 | use_trace_data_edge_detector=0 | x_ipcorerevision=6 | x_iplanguage=VERILOG
x_iplibrary=ip | x_ipname=processing_system7 | x_ipproduct=Vivado 2019.2 | x_ipsimlanguage=MIXED
x_ipvendor=xilinx.com | x_ipversion=5.5

report_drc
command_line_options
-append=default::[not_specified] | -checks=default::[not_specified] | -fail_on=default::[not_specified] | -force=default::[not_specified]
-format=default::[not_specified] | -internal=default::[not_specified] | -internal_only=default::[not_specified] | -messages=default::[not_specified]
-name=default::[not_specified] | -no_waivers=default::[not_specified] | -return_string=default::[not_specified] | -ruledecks=default::[not_specified]
-upgrade_cw=default::[not_specified] | -waived=default::[not_specified]

report_methodology
command_line_options
-append=default::[not_specified] | -checks=default::[not_specified] | -fail_on=default::[not_specified] | -force=default::[not_specified]
-format=default::[not_specified] | -messages=default::[not_specified] | -name=default::[not_specified] | -return_string=default::[not_specified]
-slack_lesser_than=default::[not_specified] | -waived=default::[not_specified]

report_power
command_line_options
-advisory=default::[not_specified] | -append=default::[not_specified] | -file=[specified] | -format=default::text
-hier=default::power | -hierarchical_depth=default::4 | -l=default::[not_specified] | -name=default::[not_specified]
-no_propagation=default::[not_specified] | -return_string=default::[not_specified] | -rpx=[specified] | -verbose=default::[not_specified]
-vid=default::[not_specified] | -xpe=default::[not_specified]
usage
airflow=250 (LFM) | ambient_temp=25.0 (C) | bi-dir_toggle=12.500000 | bidir_output_enable=1.000000
board_layers=8to11 (8 to 11 Layers) | board_selection=medium (10"x10") | clocks=0.001797 | confidence_level_clock_activity=High
confidence_level_design_state=High | confidence_level_device_models=High | confidence_level_internal_activity=Medium | confidence_level_io_activity=High
confidence_level_overall=Medium | customer=TBD | customer_class=TBD | devstatic=0.137318
die=xc7z020clg400-1 | dsp_output_toggle=12.500000 | dynamic=1.403790 | effective_thetaja=11.5
enable_probability=0.990000 | family=zynq | ff_toggle=12.500000 | flow_state=routed
heatsink=none | input_toggle=12.500000 | junction_temp=42.8 (C) | logic=0.001505
mgtavcc_dynamic_current=0.000000 | mgtavcc_static_current=0.000000 | mgtavcc_total_current=0.000000 | mgtavcc_voltage=1.000000
mgtavtt_dynamic_current=0.000000 | mgtavtt_static_current=0.000000 | mgtavtt_total_current=0.000000 | mgtavtt_voltage=1.200000
mgtvccaux_dynamic_current=0.000000 | mgtvccaux_static_current=0.000000 | mgtvccaux_total_current=0.000000 | mgtvccaux_voltage=1.800000
netlist_net_matched=NA | off-chip_power=0.000000 | on-chip_power=1.541108 | output_enable=1.000000
output_load=5.000000 | output_toggle=12.500000 | package=clg400 | pct_clock_constrained=1.000000
pct_inputs_defined=0 | platform=nt64 | process=typical | ps7=1.398874
ram_enable=50.000000 | ram_write=50.000000 | read_saif=False | set/reset_probability=0.000000
signal_rate=False | signals=0.001613 | simulation_file=None | speedgrade=-1
static_prob=False | temp_grade=commercial | thetajb=7.4 (C/W) | thetasa=0.0 (C/W)
toggle_rate=False | user_board_temp=25.0 (C) | user_effective_thetaja=11.5 | user_junc_temp=42.8 (C)
user_thetajb=7.4 (C/W) | user_thetasa=0.0 (C/W) | vccadc_dynamic_current=0.000000 | vccadc_static_current=0.020000
vccadc_total_current=0.020000 | vccadc_voltage=1.800000 | vccaux_dynamic_current=0.000000 | vccaux_io_dynamic_current=0.000000
vccaux_io_static_current=0.000000 | vccaux_io_total_current=0.000000 | vccaux_io_voltage=1.800000 | vccaux_static_current=0.014632
vccaux_total_current=0.014632 | vccaux_voltage=1.800000 | vccbram_dynamic_current=0.000000 | vccbram_static_current=0.000841
vccbram_total_current=0.000841 | vccbram_voltage=1.000000 | vccint_dynamic_current=0.004916 | vccint_static_current=0.013879
vccint_total_current=0.018795 | vccint_voltage=1.000000 | vcco12_dynamic_current=0.000000 | vcco12_static_current=0.000000
vcco12_total_current=0.000000 | vcco12_voltage=1.200000 | vcco135_dynamic_current=0.000000 | vcco135_static_current=0.000000
vcco135_total_current=0.000000 | vcco135_voltage=1.350000 | vcco15_dynamic_current=0.000000 | vcco15_static_current=0.000000
vcco15_total_current=0.000000 | vcco15_voltage=1.500000 | vcco18_dynamic_current=0.000000 | vcco18_static_current=0.000000
vcco18_total_current=0.000000 | vcco18_voltage=1.800000 | vcco25_dynamic_current=0.000000 | vcco25_static_current=0.000000
vcco25_total_current=0.000000 | vcco25_voltage=2.500000 | vcco33_dynamic_current=0.000000 | vcco33_static_current=0.000000
vcco33_total_current=0.000000 | vcco33_voltage=3.300000 | vcco_ddr_dynamic_current=0.411213 | vcco_ddr_static_current=0.002000
vcco_ddr_total_current=0.413213 | vcco_ddr_voltage=1.350000 | vcco_mio0_dynamic_current=0.001750 | vcco_mio0_static_current=0.001000
vcco_mio0_total_current=0.002750 | vcco_mio0_voltage=3.300000 | vcco_mio1_dynamic_current=0.002187 | vcco_mio1_static_current=0.001000
vcco_mio1_total_current=0.003187 | vcco_mio1_voltage=1.800000 | vccpaux_dynamic_current=0.051122 | vccpaux_static_current=0.010330
vccpaux_total_current=0.061452 | vccpaux_voltage=1.800000 | vccpint_dynamic_current=0.717025 | vccpint_static_current=0.028467
vccpint_total_current=0.745492 | vccpint_voltage=1.000000 | vccpll_dynamic_current=0.013878 | vccpll_static_current=0.003000
vccpll_total_current=0.016878 | vccpll_voltage=1.800000 | version=2019.2

report_utilization
clocking
bufgctrl_available=32 | bufgctrl_fixed=0 | bufgctrl_used=1 | bufgctrl_util_percentage=3.13
bufhce_available=72 | bufhce_fixed=0 | bufhce_used=0 | bufhce_util_percentage=0.00
bufio_available=16 | bufio_fixed=0 | bufio_used=0 | bufio_util_percentage=0.00
bufmrce_available=8 | bufmrce_fixed=0 | bufmrce_used=0 | bufmrce_util_percentage=0.00
bufr_available=16 | bufr_fixed=0 | bufr_used=0 | bufr_util_percentage=0.00
mmcme2_adv_available=4 | mmcme2_adv_fixed=0 | mmcme2_adv_used=0 | mmcme2_adv_util_percentage=0.00
plle2_adv_available=4 | plle2_adv_fixed=0 | plle2_adv_used=0 | plle2_adv_util_percentage=0.00
dsp
dsps_available=220 | dsps_fixed=0 | dsps_used=0 | dsps_util_percentage=0.00
io_standard
blvds_25=0 | diff_hstl_i=0 | diff_hstl_i_18=0 | diff_hstl_ii=0
diff_hstl_ii_18=0 | diff_hsul_12=0 | diff_mobile_ddr=0 | diff_sstl135=1
diff_sstl135_r=0 | diff_sstl15=0 | diff_sstl15_r=0 | diff_sstl18_i=0
diff_sstl18_ii=0 | hstl_i=0 | hstl_i_18=0 | hstl_ii=0
hstl_ii_18=0 | hsul_12=0 | lvcmos12=0 | lvcmos15=0
lvcmos18=1 | lvcmos25=0 | lvcmos33=1 | lvds_25=0
lvttl=0 | mini_lvds_25=0 | mobile_ddr=0 | pci33_3=0
ppds_25=0 | rsds_25=0 | sstl135=1 | sstl135_r=0
sstl15=0 | sstl15_r=0 | sstl18_i=0 | sstl18_ii=0
tmds_33=0
memory
block_ram_tile_available=140 | block_ram_tile_fixed=0 | block_ram_tile_used=0 | block_ram_tile_util_percentage=0.00
ramb18_available=280 | ramb18_fixed=0 | ramb18_used=0 | ramb18_util_percentage=0.00
ramb36_fifo_available=140 | ramb36_fifo_fixed=0 | ramb36_fifo_used=0 | ramb36_fifo_util_percentage=0.00
primitives
bibuf_functional_category=IO | bibuf_used=130 | bufg_functional_category=Clock | bufg_used=1
carry4_functional_category=CarryLogic | carry4_used=60 | fdre_functional_category=Flop & Latch | fdre_used=682
fdse_functional_category=Flop & Latch | fdse_used=19 | lut1_functional_category=LUT | lut1_used=15
lut2_functional_category=LUT | lut2_used=118 | lut3_functional_category=LUT | lut3_used=281
lut4_functional_category=LUT | lut4_used=125 | lut5_functional_category=LUT | lut5_used=67
lut6_functional_category=LUT | lut6_used=160 | ps7_functional_category=Specialized Resource | ps7_used=1
srl16e_functional_category=Distributed Memory | srl16e_used=19 | srlc32e_functional_category=Distributed Memory | srlc32e_used=45
slice_logic
f7_muxes_available=26600 | f7_muxes_fixed=0 | f7_muxes_used=0 | f7_muxes_util_percentage=0.00
f8_muxes_available=13300 | f8_muxes_fixed=0 | f8_muxes_used=0 | f8_muxes_util_percentage=0.00
lut_as_distributed_ram_fixed=0 | lut_as_distributed_ram_used=0 | lut_as_logic_available=53200 | lut_as_logic_fixed=0
lut_as_logic_used=595 | lut_as_logic_util_percentage=1.12 | lut_as_memory_available=17400 | lut_as_memory_fixed=0
lut_as_memory_used=60 | lut_as_memory_util_percentage=0.34 | lut_as_shift_register_fixed=0 | lut_as_shift_register_used=60
register_as_flip_flop_available=106400 | register_as_flip_flop_fixed=0 | register_as_flip_flop_used=701 | register_as_flip_flop_util_percentage=0.66
register_as_latch_available=106400 | register_as_latch_fixed=0 | register_as_latch_used=0 | register_as_latch_util_percentage=0.00
slice_luts_available=53200 | slice_luts_fixed=0 | slice_luts_used=655 | slice_luts_util_percentage=1.23
slice_registers_available=106400 | slice_registers_fixed=0 | slice_registers_used=701 | slice_registers_util_percentage=0.66
lut_as_distributed_ram_fixed=0 | lut_as_distributed_ram_used=0 | lut_as_logic_available=53200 | lut_as_logic_fixed=0
lut_as_logic_used=595 | lut_as_logic_util_percentage=1.12 | lut_as_memory_available=17400 | lut_as_memory_fixed=0
lut_as_memory_used=60 | lut_as_memory_util_percentage=0.34 | lut_as_shift_register_fixed=0 | lut_as_shift_register_used=60
lut_in_front_of_the_register_is_unused_fixed=60 | lut_in_front_of_the_register_is_unused_used=167 | lut_in_front_of_the_register_is_used_fixed=167 | lut_in_front_of_the_register_is_used_used=56
register_driven_from_outside_the_slice_fixed=56 | register_driven_from_outside_the_slice_used=223 | register_driven_from_within_the_slice_fixed=223 | register_driven_from_within_the_slice_used=478
slice_available=13300 | slice_fixed=0 | slice_registers_available=106400 | slice_registers_fixed=0
slice_registers_used=701 | slice_registers_util_percentage=0.66 | slice_used=252 | slice_util_percentage=1.89
slicel_fixed=0 | slicel_used=150 | slicem_fixed=0 | slicem_used=102
unique_control_sets_available=13300 | unique_control_sets_fixed=13300 | unique_control_sets_used=46 | unique_control_sets_util_percentage=0.35
using_o5_and_o6_fixed=0.35 | using_o5_and_o6_used=4 | using_o5_output_only_fixed=4 | using_o5_output_only_used=0
using_o6_output_only_fixed=0 | using_o6_output_only_used=56
specific_feature
bscane2_available=4 | bscane2_fixed=0 | bscane2_used=0 | bscane2_util_percentage=0.00
capturee2_available=1 | capturee2_fixed=0 | capturee2_used=0 | capturee2_util_percentage=0.00
dna_port_available=1 | dna_port_fixed=0 | dna_port_used=0 | dna_port_util_percentage=0.00
efuse_usr_available=1 | efuse_usr_fixed=0 | efuse_usr_used=0 | efuse_usr_util_percentage=0.00
frame_ecce2_available=1 | frame_ecce2_fixed=0 | frame_ecce2_used=0 | frame_ecce2_util_percentage=0.00
icape2_available=2 | icape2_fixed=0 | icape2_used=0 | icape2_util_percentage=0.00
startupe2_available=1 | startupe2_fixed=0 | startupe2_used=0 | startupe2_util_percentage=0.00
xadc_available=1 | xadc_fixed=0 | xadc_used=0 | xadc_util_percentage=0.00

synthesis
command_line_options
-assert=default::[not_specified] | -bufg=default::12 | -cascade_dsp=default::auto | -constrset=default::[not_specified]
-control_set_opt_threshold=default::auto | -directive=default::default | -fanout_limit=default::10000 | -flatten_hierarchy=default::rebuilt
-fsm_extraction=default::auto | -gated_clock_conversion=default::off | -generic=default::[not_specified] | -include_dirs=default::[not_specified]
-keep_equivalent_registers=default::[not_specified] | -max_bram=default::-1 | -max_bram_cascade_height=default::-1 | -max_dsp=default::-1
-max_uram=default::-1 | -max_uram_cascade_height=default::-1 | -mode=default::default | -name=default::[not_specified]
-no_lc=default::[not_specified] | -no_srlextract=default::[not_specified] | -no_timing_driven=default::[not_specified] | -part=xc7z020clg400-1
-resource_sharing=default::auto | -retiming=default::[not_specified] | -rtl=default::[not_specified] | -rtl_skip_constraints=default::[not_specified]
-rtl_skip_ip=default::[not_specified] | -seu_protect=default::none | -sfcu=default::[not_specified] | -shreg_min_size=default::3
-top=Assignment_7_BD_wrapper | -verilog_define=default::[not_specified]
usage
elapsed=00:00:21s | hls_ip=0 | memory_gain=695.555MB | memory_peak=1176.430MB